
OWH80 Series Single-Channel Programmable DC Power Supply 

Technical Specification
The instrument must be operated continuously for more than 30 minutes at the specified operating temperature to achieve the following specifications.
	Model
	OWH80120-1800

1ch
	OWH8080-2000

1ch

	Rated output

(0℃-40℃)
	Voltage 
	0-80V
	0 -80V

	
	OVP
	1V-85V
	1V-85V

	
	Current
	0-120A
	0-80A

	
	OCP
	1A-121A
	1A-81A

	
	Power 
	1800W
	2000W

	Input power*
	Volt/freq.
	198V-240Vac*1；

45Hz-65Hz
	198V-240Vac*1；

45Hz-65Hz

	Load regulation

(%of output+offset)
	CV
	≤0.03%+20mV
	≤0.03%+20mV

	
	CC
	≤0.05%+30mA
	≤0.05%+30mA

	Input power regulation

 (%of output+offset)
	CV
	≤0.03%+20mV
	≤0.05%+20mV

	
	CC
	≤0.05%+30mA
	≤0.05%+30mA

	Setting resolution
	Voltage
	10mV
	10mV

	
	Current
	1mA
	1mA

	Readback resolution
	Voltage
	1mV
	1mV

	
	Current
	1mA
	1mA

	Setting accuracy
	Voltage
	≤0.05% ± 40mV
	≤0.05% ± 40mV

	
	Current
	≤0.1% ± 0.1%FS
	≤0.1% ± 0.1%FS

	Readback accuracy
	Voltage
	≤0.05% ± 40mV
	≤0.05% ± 40mV

	
	Current
	≤0.1% ± 0.1%FS
	≤0.1% ± 0.1%FS

	Ripple noise(*)
	Voltage
	≤100mVp-p
	≤100mVp-p

	
	Current 
	≤100mArms
	≤120mArms

	Output temp drift coefficient

(0℃-40℃)
	Voltage
	100ppm/℃
	100ppm/℃

	
	Current
	200ppm/℃
	200ppm/℃

	Readback temp drift
	Voltage
	100ppm/℃
	100ppm/℃

	
	Current
	200ppm/℃
	200ppm/℃

	Transient response (10%-90% rated load)
	≤5.0ms
	≤5.0ms

	Working temperature
	0-40℃
	0-40℃

	Display
	4.3inch TFT LCD screen

	Interface
	USB, LAN, RS485，RS232

	Dimension
	215.0mm(W) X 133.0mm(H) X 446.2mm(D)

	Weight
	Approx. 6kg
	Approx. 6kg


*1: Input voltage: 100-120Vac, output power reduced by half.
	Model
	OWH50120-1800

1ch

	Rated output

(0℃-40℃)
	Voltage 
	0-50V

	
	OVP
	1V-55V

	
	Current
	0-120A

	
	OCP
	1A-121A

	
	Power 
	1800W

	Input power*
	Volt/freq.
	100V-240Vac*1；45Hz-65Hz

	Load regulation

(%of output+offset)
	CV
	≤0.03%+20mV

	
	CC
	≤0.05%+30mA

	Input power regulation

 (%of output+offset)
	CV
	≤0.03%+20mV

	
	CC
	≤0.05%+30mA

	Setting resolution
	Voltage
	10mV

	
	Current
	1mA

	Readback resolution
	Voltage
	1mV

	
	Current
	1mA

	Setting accuracy
	Voltage
	≤0.05% ± 40mV

	
	Current
	≤0.1% ± 0.1%FS

	Readback accuracy
	Voltage
	≤0.05% ± 40mV

	
	Current
	≤0.1% ± 0.1%FS

	Ripple noise(*)
	Voltage
	≤100mVp-p

	
	Current 
	≤100mArms

	Output temp drift coefficient

(0℃-40℃)
	Voltage
	100ppm/℃

	
	Current
	200ppm/℃

	Readback temp drift
	Voltage
	100ppm/℃

	
	Current
	200ppm/℃

	Transient response (10%-90% rated load)
	≤5.0ms

	Working temperature
	0-40℃

	Display
	4.3inch TFT LCD screen

	Interface
	USB, LAN, RS485，RS232

	Size
	215.0mm(W) X 133.0mm(H) X 446.2mm(D)

	Weight
	Approx. 7kg


*1: Input voltage: 100-120Vac, output power reduced by half.
Interval Period of Adjustment: 

One year is recommended for the calibration interval period.
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